Content

[2 Classes 1](#_Toc25338349)

[2.1 AirInterfaceCapability 1](#_Toc25338350)

[2.2 AirInterfaceConfiguration 5](#_Toc25338351)

[2.3 AirInterfaceCurrentPerformance 12](#_Toc25338352)

[2.4 AirInterfaceCurrentProblems 13](#_Toc25338353)

[2.5 AirInterfaceHistoricalPerformances 14](#_Toc25338354)

[2.6 AirInterfaceLpSpec 14](#_Toc25338355)

[2.7 AirInterfaceStatus 15](#_Toc25338356)

[2.8 AirInterface\_Pac 20](#_Toc25338357)

[2.9 CurrentPerformance 21](#_Toc25338358)

[2.10 CurrentProblem 24](#_Toc25338359)

[2.11 HistoricalPerformance 25](#_Toc25338360)

[2.12 TransmissionMode 27](#_Toc25338361)

[3 Data Types 30](#_Toc25338362)

[3.1 AcmThresholdCrossAlarmType 30](#_Toc25338363)

[3.2 AirInterfaceCurrentPerformanceType 31](#_Toc25338364)

[3.3 AirInterfaceCurrentProblemType 31](#_Toc25338365)

[3.4 AirInterfaceHistoricalPerformanceType 32](#_Toc25338366)

[3.5 AirInterfacePerformanceType 32](#_Toc25338367)

[3.6 G826ThresholdCrossAlarmType 37](#_Toc25338368)

[3.7 ProblemKindSeverityType 38](#_Toc25338369)

[3.8 RadioSignalIdType 39](#_Toc25338370)

[3.9 TimeXStatesType 39](#_Toc25338371)

[3.10 XltsThresholdCrossAlarmType 40](#_Toc25338372)

[4 Enumeration Types 42](#_Toc25338373)

[4.1 AdministrativeStateType 42](#_Toc25338374)

[4.2 G826Type 42](#_Toc25338375)

[4.3 GranularityPeriodType 42](#_Toc25338376)

[4.4 InterfaceStatusType 43](#_Toc25338377)

[4.5 LayerProtocolNameType 43](#_Toc25338378)

[4.6 LoopBackType 43](#_Toc25338379)

[4.7 OperationalStateType 44](#_Toc25338380)

[4.8 RadioSignalIdDatatypeType 44](#_Toc25338381)

[4.9 SeverityType 44](#_Toc25338382)

[4.10 XLevelThresholdSecondKindType 44](#_Toc25338383)

[5 Primitive Types 45](#_Toc25338384)

# Classes

## AirInterfaceCapability

Describes the 'analog' capabilities of modem and transmitter of the microwave device. Value ranges of attributes are not independently (e.g. min. and max. transmit power depends on modulation). Legal combinations of values are expressed in transmissionModeTypes.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceCapability

Table 1: Attributes for AirInterfaceCapability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| typeOfEquipment | String  Type of equipment not yet defined. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | This parameter indicates the equipment type. Instead of uploading the complete set of capabilities, capabilities of the same equipment type could be reused. Should be unique for a combination of modem, radio and their respective firmware. |
| txFrequencyMin | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Value of the minimum transmit frequency tunable at the air interface. |
| txFrequencyMax | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Value of the maximum transmit frequency tunable at the air interface. |
| rxFrequencyMin | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Value of the minimum receive frequency tunable at the air interface. |
| rxFrequencyMax | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Value of the maximum receive frequency tunable at the air interface. |
| \_transmissionModeList | TransmissionMode  ./. | 1..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | List of supported Transmission Modes. |
| duplexDistanceIsFreelyConfigurable | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | 1 = Transmitted and received frequency can be freely chosen between the given minimum and maximum values. |
| duplexDistanceList | Integer  -1 | 1..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Only relevant if (duplexDistanceIsFreelyConfigurable==0). Lists all supported distances between transmitted and received frequency. |
| autoFreqSelectIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | In case the microwave radio is capable of automatically selecting the transmit frequency in unlicensed bands, this field shall contain a 'true'. |
| adaptiveModulationIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | In case the device is capable of adaptive modulation, this field shall contain a 'true'. |
| atpcIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | In case the microwave radio is capable of ATPC, this field shall contain a 'true'. |
| atpcRange | Integer  0 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dB  • support: MANDATORY | Extent of the ATPC range. This value represents a device specific maximum value. The actual range of the ATPC at a specific link might be limited by the difference between configured transmit power (AirInterface::AirInterfaceConfiguration::txPower) and minimum transmit power of the device (TypeDefinitions::TransmissionModeType::txPowerMin). |
| supportedRadioSignalIdDatatype | RadioSignalIdDatatypeType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | This attribute is for expressing the datatype, which is supported as a Radio Signal ID by the device. |
| supportedRadioSignalIdLength | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If (supportedRadioSignalIdDatatype==INTEGER): Maximum value of the Radio Signal ID supported by the device; If (supportedRadioSignalIdDatatype==STRING): Maximum number of letters supported by the device. |
| expectedEqualsTransmittedRadioSignalID | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | 1 = It is not possible to configure an expectedRadioSignalID different from the transmittedRadioSignalID. |
| encryptionIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Shall be marked 'true', if payload encryption is available. |
| supportedLoopBackKindList | LoopBackType  NONE | 1..4 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | List of supported kinds of looping back of header information to the remote site. |
| maintenanceTimerRange | String  Range of the maintenance timer not yet defined. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Available time periods for maintenance configurations (e.g. the loop back of microwave header information) to be described. Concrete values shall be separated by commas (e.g. '10, 60, 360'). Ranges shall be expressed as two values separated by a minus (e.g. '10-360'). |
| supportedAlarmList | String  Supported alarms not yet defined. | 7..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Available alarms to be listed. Mandatory:'signalIsLost','rslIsExceeded','signalIDMismatching','temperatureIsExceeded','modemIsFaulty','radioIsFaulty' and 'modulationIsDownShifted'. Further alarms might be added by the vendor. |
| performanceMonitoringIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | 1 = Collection and aggregation of performance values is available. |

## AirInterfaceConfiguration

Configuration of the radio link.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceConfiguration

Table 1: Attributes for AirInterfaceConfiguration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| airInterfaceName | String  Air interface ID not yet defined. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Operator specific microwave link ID (often used for coding area, type of element and sequential number). |
| remoteAirInterfaceName | String  Air interface ID at the remote site not yet defined. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Name of the air interface, which belongs to the same link, at the remote site. |
| transmittedRadioSignalID | RadioSignalIdType  ./. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Transmitted radio signal ID for synchronizing the remote receiver. |
| expectedRadioSignalID | RadioSignalIdType  ./. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Received radio signal ID for identifying the correct transmitter to synchronize on. |
| txFrequency | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Center frequency of the transmit channel. The values to be configured have to exactly match the values listed in the international agreement referenced in channelPlanID. In case of automated selection of the transmit frequency this field shall describe the lowest center frequency selectable. |
| rxFrequency | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Center frequency of the receive channel. |
| \_transmissionModeMin | TransmissionMode  ./. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  PassedByReference | Minimum transmission mode to be configured (in case adaptive modulation is not used, this value represents also the fixed transmission mode). |
| \_transmissionModeMax | TransmissionMode  ./. | 0..1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  PassedByReference | Maximum transmission mode to be configured. |
| powerIsOn | Boolean  true | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Power ON. Activation of the entire radio in a split mount configuration shall be expressed as a 'true'. |
| transmitterIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activation of the transmitter inside the radio shall be expressed as a 'true'. |
| receiverIsOn | Boolean  true | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Maintenance Feature. Activation of the receiver inside the radio shall be expressed as a 'true'. Attribute shall also be used for RX main and RX diversity squelches in case of diversity configurations. |
| txPower | Integer  99 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Transmit power to be configured on the microwave link. Signed Byte is required. The actually operated transmit power might be lower depending on adaptive modulation and ATPC. |
| adaptiveModulationIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Adaptive Modulation. Activation of adaptive modulation shall be expressed as a 'true'. |
| xpicIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activation of Cross Polarization Interference Cancelation shall be expressed as a 'true'. In case XPIC is not available for the current combination of channel bandwidth and modulation or the hardware in general, this parameter shall always be set to 'false'. |
| mimoIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activation of Multiple Input Multiple Output (MIMO) shall be expressed as a 'true'. |
| alicIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activation of Adjacent Link Interference Cancelation (ALIC) shall be expressed as a 'true'. |
| atpcIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | ATPC. Activation of Automated Transmit Power Control shall be expressed as a 'true'. |
| atpcThreshUpper | Integer  99 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | If the receive level is higher than the upper threshold value, the transmitter is notified to decrease transmit power. |
| atpcThreshLower | Integer  99 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | If the receive level is lower than the lower threshold value, the transmitter is notified to increase transmit power. |
| atpcTxPowerMin | Integer  -99 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Transmit power, which is not to be undercut, while operating ATPC. |
| autoFreqSelectIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activation of automatically selecting the transmit frequency in unlicensed bands shall be expressed as a 'true'. |
| autoFreqSelectRange | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: channels  • support: MANDATORY | Number of transmit channels (starting at the center frequency defined in txFrequency and with channel bandwidth according to txChannelBandwidth) that define the range within the transmit frequency can automatically been chosen. |
| modulationIsOn | Boolean  true | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Maintenance Feature. De-activation of the modulation of the carrier signal for fault management shall be expressed as a 'false'. |
| encryptionIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Activates encryption of the payload. |
| cryptographicKey | String  Cryptographic key not yet defined. | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Key for transforming plaintext into ciphertext data. |
| loopBackKindOn | LoopBackType  NONE | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Maintenance Feature. The currently configured type of looping back of the air interface header shall be expressed here. The received header is returned to the remote site. |
| maintenanceTimer | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: s  • support: MANDATORY | Time of existence of any maintenance configuration (e.g. the loop back of microwave header information). 0 = maintenance timer is switched off. Valid values are defined in AirInterface::AirInterfaceCapability::maintenanceTimerRange. |
| problemKindSeverityList | ProblemKindSeverityType  ./. | 6..\* | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Severity of the problem to be configured. |
| g826ThresholdCrossAlarmList | G826ThresholdCrossAlarmType  ./. | 0..6 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | List of G826 related threshold cross alarms to be configured. |
| xltsThresholdCrossAlarmList | XltsThresholdCrossAlarmType  ./. | 0..\* | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | List of RLTS or TLTS (ETSI ETSI EN 301 129) related threshold cross alarms to be configured. |
| acmThresholdCrossAlarmList | AcmThresholdCrossAlarmType  ./. | 0..\* | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | List threshold cross alarms, which relate to the time period of operation of a specific transmission mode. |
| clearingThresholdCrossAlarmsIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Setting this bit is clearing all the currently active threshold cross alarms. |
| performanceMonitoringIsOn | Boolean  false | 1 | RW | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Enables measurement, collection, storage and access to performance data. |

## AirInterfaceCurrentPerformance

Aggregated performance information of the air interface at a particular moment.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceCurrentPerformance

Table 1: Attributes for AirInterfaceCurrentPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| currentPerformanceDataList | AirInterfaceCurrentPerformanceType  ./. | 1..2 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | At least values of the counters, which are reset every 15 minutes, are to be provided. If available, the current values of the counters, which are reset every 24 hour, can be provided, too. |

## AirInterfaceCurrentProblems

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceCurrentProblems

Table 1: Attributes for AirInterfaceCurrentProblems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| currentProblemList | AirInterfaceCurrentProblemType  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |

## AirInterfaceHistoricalPerformances

Aggregated performance information of the air interface for a pre-defined measurement interval.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceHistoricalPerformances

Table 1: Attributes for AirInterfaceHistoricalPerformances

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| historicalPerformanceDataList | AirInterfaceHistoricalPerformanceType  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |

## AirInterfaceLpSpec

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: YES
* objectDeletionNotification: YES
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceLpSpec

Table 1: Attributes for AirInterfaceLpSpec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_airInterface\_Pac | AirInterface\_Pac  ./. | 1 | RW | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |

## AirInterfaceStatus

Measurements of current values on the air interface and operational status of the device.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterfaceStatus

Table 1: Attributes for AirInterfaceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| interfaceStatus | InterfaceStatusType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Operational status of the interface. |
| txFrequencyCur | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Center frequency of the currently operated transmit channel. |
| rxFrequencyCur | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Center frequency of the currently operated receive channel. |
| \_transmissionModeCur | TransmissionMode  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  PassedByReference | Currently operated transmission mode according to definitions in Capabilities. |
| receivedRadioSignalID | RadioSignalIdType  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Radio signal ID of the signal, which the receiver is currently synchronized on. |
| radioPowerIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If the radio unit has power and is switched on, this shall be expressed as a 'true'. |
| linkIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If connection is established to the remote site with the same linkID, this shall be expressed as a 'true'. |
| xpicIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If XPIC is currently actually working (not just configured), this shall be expressed as a 'true'. |
| mimoIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If MIMO is currently actually working (not just configured), this shall be expressed as a 'true'. |
| alicIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If Adjacent Link Interference Cancelation (ALIC) is currently actually working (not just configured), this shall be expressed as a 'true'. |
| atpcIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If ATPC is currently actually working (not just configured), this shall be expressed as a 'true'. |
| autoFreqSelectIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | If automated frequency selection is currently actually working (not just configured), this shall be expressed as a 'true'. |
| localEndPointId | String  not-supported | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | The value of the localEndPointId is a vendor specific identifier of the air interface, used by the node to discover a microwave radio link. |
| remoteEndPointId | String  not-supported | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | The value of the remoteEndPointId is a vendor specific identifier of the airinterface at the remote side, used to by the node to discover a microwave radio link. |
| loopBackKindUp | LoopBackType  NONE | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | The currently active (not just configured) type of looping back of the air interface header shall be expressed here. The received header is returned to the remote site. |
| performanceMonitoringIsUp | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | 1 = Performance values are currently collected and aggregated. |
| rxLevelCur | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Current receive level. |
| txLevelCur | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Current transmit level. |
| snirCur | Integer  -99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dB  • support: MANDATORY | Currently measured signal to (noise+interference) ratio. |
| xpdCur | Integer  -99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: dB  • support: MANDATORY | Currently measured cross polarization discrimination. |
| rfTempCur | Integer  -99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: Celsius  • support: MANDATORY | Current temperature (in degree Celsius) of the radio module inside the outdoor unit. |

## AirInterface\_Pac

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for AirInterface\_Pac

Table 1: Attributes for AirInterface\_Pac

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_airInterfaceCapability | AirInterfaceCapability  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |
| \_airInterfaceConfiguration | AirInterfaceConfiguration  ./. | 1 | RW | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |
| \_airInterfaceStatus | AirInterfaceStatus  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |
| \_airInterfaceCurrentProblems | AirInterfaceCurrentProblems  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |
| \_airInterfaceCurrentPerformance | AirInterfaceCurrentPerformance  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |
| \_airInterfaceHistoricalPerformances | AirInterfaceHistoricalPerformances  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | See referenced class |

## CurrentPerformance

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for CurrentPerformance

Table 1: Attributes for CurrentPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| timestamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | The timestamp associated with when the current data was collected. |
| suspectIntervalFlag | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | This attribute is used to indicate that the performance data for the current period may not be reliable. Some reasons for this to occur are: – Suspect data were detected by the actual resource doing data collection. – Transition of the administrativeState attribute to/from the 'lock' state. – Transition of the operationalState to/from the 'disabled' state. – Scheduler setting that inhibits the collection function. – The performance counters were reset during the interval. – The currentData (or subclass) object instance was created during the monitoring period. |
| elapsedTime | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_64\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: s  • support: MANDATORY | Number of seconds that elapsed since the last reset of the counter. |
| scannerId | String  Scanner ID not defined. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| operationalState | OperationalStateType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| granularityPeriod | GranularityPeriodType  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Time period between reset of the underlying counter. |
| administrativeState | AdministrativeStateType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| objectClass | ObjectIdentifier  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | ObjectClass ::= CHOICE{ globalForm [0] OBJECT IDENTIFIER, localForm [1] INTEGER} |
| nameBinding | ObjectIdentifier  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| packages | ObjectIdentifier  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| allomorphs | ObjectIdentifier  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |

## CurrentProblem

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for CurrentProblem

Table 1: Attributes for CurrentProblem

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| sequenceNumber | Integer  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Unique sequence number of the current problem object. |
| timestamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| problemSeverity | SeverityType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Severity of the alarm. |

## HistoricalPerformance

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HistoricalPerformance

Table 1: Attributes for HistoricalPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| suspectIntervalFlag | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | This attribute indicates that the data collected during the interval is suspect. |
| historyDataId | String  History Data ID not defined. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| periodEndTime | DateTime  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 2  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Time when the counter values have been recorded and the counter reset. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Time period between reset of the underlying counter. |
| objectClass | ObjectIdentifier  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | ObjectClass ::= CHOICE{ globalForm [0] OBJECT IDENTIFIER, localForm [1] INTEGER} |
| nameBinding | ObjectIdentifier  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| packages | ObjectIdentifier  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |
| allomorphs | ObjectIdentifier  ./. | 0..\* | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY |  |

## TransmissionMode

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for TransmissionMode

Table 1: Attributes for TransmissionMode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| transmissionModeName | String  ./. | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Name of the transmission mode. BBBB-m\*-i\*/t\*-r\*. B=four digits of channel bandwidth in MHz. m\*=required number of digits for modulation name. (i\*/t\*=code rate.) i\*=required number of digits for number of information bits. t\*=required number of digits for total bits. r\*=required number of digits for rate reduction factor. Example: 0028-4QAM-188/204-1 |
| transmissionModeRank | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Configuring adaptive modulation by selecting \_transmissionModeMin and \_transmissionModeMin requires the transmission modes to be ordered. The vendor shall rank all available transmission modes according to the respective payload data rate. The application providers shall order the transmission modes according to the rank. |
| channelBandwidth | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kHz  • support: MANDATORY | Bandwidth of the transmit channel. The value shall be expressed explicitly (means in kHz) not as a reference to an international agreement. The values shall be chosen from the following \_list: 3.500, 7.000, 14.000, 27.500, 28.000, 29.000, 29.650, 30.000, 40.000, 50.000, 55.000, 56.000, 59.300, 60.000, 80.000, 100.000, 112.000, 120.000, 150.000, 200.000, 250.000, 500.000, 750.000, 1.000.000, 1.250.000, 1.500.000, 1.750.000, 2.000.000; |
| modulationScheme | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: symbols  • support: MANDATORY | Modulation scheme, which is base to the other characteristics described in the same transmissionModeType data type. The modulation scheme shall be described by the number of states in the phase diagram (e.g. BPSK->'2' or 256QAM->'256'). |
| codeRate | Integer  -1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: %  • support: MANDATORY | Code rate of the coding scheme in % (Net bit rate ≤ Gross bit rate · code rate). |
| symbolRateReductionFactor | Integer  1 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | Reduction factor for the symbol rate. Example: value would be 4 for 1/4BPSK. |
| txPowerMin | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Value of the minimum transmit power the modem can operate in dBm. |
| txPowerMax | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Value of the maximum transmit power the modem can operate in dBm. |
| rxThreshold | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_16\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Value of the receive level required to decode the received signal with a Bit Error Rate of 1e-6 or less. |
| amUpshiftLevel | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Value of the receive level that has to be exceeded to shift into a higher modulation scheme. |
| amDownshiftLevel | Integer  99 | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: dBm  • support: MANDATORY | Value of the receive level that has to be exceeded for not shifting into a lower modulation scheme. |
| xpicIsAvail | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | In case this air interface type is capable of XPIC, this field shall contain a 'true'. This information shall purely relate to capabilities of the equipment type, but not to the operational capability of a specific hardware composition on site. Means for example that this attribute might contain a 'true' statement, even if an additional cable would have been required to actually operate XPIC in a specific case. |
| supportedAsFixedConfiguration | Boolean  false | 1 | R | OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA  OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY | 1 = This transmission mode is available for manual configuration when Adaptive Modulation is switched off. |

# Data Types

## AcmThresholdCrossAlarmType

Applied Stereotypes:

Attributes for AcmThresholdCrossAlarmType

Table 1: Attributes for AcmThresholdCrossAlarmType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| acmThresholdCrossAlarmDefinitionNumber | Integer  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Sequence number of the definitions. |
| \_transmissionMode | TransmissionMode  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   PassedByReference |  |
| amountOfSeconds | Integer  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_16\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY | Number of seconds, in which the referenced transmission mode has to be operated until the threshold cross alarm is raised for this 15min or 24hour period. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 2 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Period of the performance data collection. |

## AirInterfaceCurrentPerformanceType

Turns performance information into current performance information by inheriting from OTN\_CurrentData.

Applied Stereotypes:

Attributes for AirInterfaceCurrentPerformanceType

Table 1: Attributes for AirInterfaceCurrentPerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| performanceData | AirInterfacePerformanceType  ./. | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY |  |

## AirInterfaceCurrentProblemType

Applied Stereotypes:

Attributes for AirInterfaceCurrentProblemType

Table 1: Attributes for AirInterfaceCurrentProblemType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| problemName | String  Problem name not specified. | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Name of the alarm according to AirInterface::AirInterfaceCapability::supportedAlarms |

## AirInterfaceHistoricalPerformanceType

Turns performance information into historical performance information by inheriting from OTN\_HistoryData.

Applied Stereotypes:

Attributes for AirInterfaceHistoricalPerformanceType

Table 1: Attributes for AirInterfaceHistoricalPerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| performanceData | AirInterfacePerformanceType  ./. | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY |  |

## AirInterfacePerformanceType

Consolidated performance information of the air interface.

Applied Stereotypes:

Attributes for AirInterfacePerformanceType

Table 1: Attributes for AirInterfacePerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| es | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Number of errored seconds. |
| ses | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Number of severely errored seconds. |
| cses | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Number of consecutive severely errored seconds. |
| unavailability | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Total time of unavailability in seconds. |
| txLevelMin | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Minimum transmit power. Signed integers are required. |
| txLevelMax | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Maximum transmit power. Signed integers are required. |
| txLevelAvg | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Averaged transmit power. Signed integers are required. |
| rxLevelMin | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Minimum receive level. Signed integers are required. |
| rxLevelMax | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Maximum receive level. Signed integers are required. |
| rxLevelAvg | Integer  99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | Averaged receive level. Signed integers are required. |
| timeXStatesList | TimeXStatesType  ./. | 1..\* | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Time period the transmitter operated in the respective transmission mode. |
| snirMin | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Minimum signal to (noise+interference) ratio. |
| snirMax | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Maximum signal to (noise+interference) ratio. |
| snirAvg | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Averaged signal to (noise+interference) ratio. |
| xpdMin | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Minimum cross polarization discrimination. |
| xpdMax | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Maximum cross polarization discrimination. |
| xpdAvg | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dB * support: MANDATORY | Averaged cross polarization discrimination. |
| rfTempMin | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: Celsius * support: MANDATORY | Lowest temperature (in degree Celsius) of the radio module inside the outdoor unit. |
| rfTempMax | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: Celsius * support: MANDATORY | Highest temperature (in degree Celsius) of the radio module inside the outdoor unit. |
| rfTempAvg | Integer  -99 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: Celsius * support: MANDATORY | Averaged temperature (in degree Celsius) of the radio module inside the outdoor unit. |
| defectBlocksSum | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_16\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: blocks * support: MANDATORY | Total number of blocks that were defect after receiving and could not be corrected by the FEC. |
| timePeriod | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Total length of the measurement period. |

## G826ThresholdCrossAlarmType

Allows defining a threshold cross alarm.

Applied Stereotypes:

Attributes for G826ThresholdCrossAlarmType

Table 1: Attributes for G826ThresholdCrossAlarmType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| g826ValueKind | G826Type  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Kind of performance value that shall be equipped with a threshold alarm. |
| alarmRaisingThreshold | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY | Number of events required for raising the threshold cross alarm. |
| alarmClearingThreshold | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY | Number of events required for clearing the threshold cross alarm. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 2 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Period of the performance data collection. |

## ProblemKindSeverityType

Applied Stereotypes:

Attributes for ProblemKindSeverityType

Table 1: Attributes for ProblemKindSeverityType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| problemKindName | String  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Name of the alarm according to supportedAlarmList |
| problemKindSeverity | SeverityType  NOT\_YET\_DEFINED | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Severity of this type of alarm. |

## RadioSignalIdType

Applied Stereotypes:

Attributes for RadioSignalIdType

Table 1: Attributes for RadioSignalIdType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| numericRadioSignalID | Integer  0 | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_16\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Only relevant if (supportedRadioSignalIdDatatype==INTEGER): 0 = the receiver ignores the signal ID of the received signal. Any other value = the receiver exclusively synchronizes on signals with the same signal ID. |
| alphanumericRadioSignalID | String  Not yet defined. | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Only relevant if (supportedRadioSignalIdDatatype==STRING): Empty field = the receiver ignores the signal ID of the received signal. Any other entry = the receiver exclusively synchronizes on signals with the same signal ID. |

## TimeXStatesType

Applied Stereotypes:

Attributes for TimeXStatesType

Table 1: Attributes for TimeXStatesType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| timeXStateSequenceNumber | Integer  ./. | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Sequence number of the performance value. |
| \_transmissionMode | TransmissionMode  ./. | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   PassedByReference | Operated transmission mode. |
| time | Integer  -1 | 1 | R | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY | Sum of all seconds the transmitter operated the transmission mode. |

## XltsThresholdCrossAlarmType

Applied Stereotypes:

Attributes for XltsThresholdCrossAlarmType

Table 1: Attributes for XltsThresholdCrossAlarmType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| levelThresholdSecondKind | XLevelThresholdSecondKindType  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Defines whether receive (RLTS) or transmit (TLTS) level triggers the threshold cross alarm. |
| xltsLevel | Integer  ./. | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT   OpenModelAttribute   * partOfObjectKey: 3 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY | If (LevelThresholdSecondKindType==RLTS): Receive level, which has to be undercut, for the performance counter incrementing the number of seconds. If (LevelThresholdSecondKindType==TLTS): Transmit level, which has to be exceeded, for the performance counter incrementing the number of seconds. See also ETSI EN 301 129 V1.1.2 (1999-05). |
| amountOfSeconds | Integer  -1 | 1 | RW | OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_16\_BIT   OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY | Number of seconds, which has to be exceeded for causing the threshold cross alarm to raise for this period. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | RW | OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA   OpenModelAttribute   * partOfObjectKey: 2 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY | Period of the performance data collection. |

# Enumeration Types

## AdministrativeStateType

For more information on Administrative State, See ITU-T Recs. X.731 and M.3100.

Contains Enumeration Literals:

* UNLOCKED:
* LOCKED:
* SHUTTING\_DOWN:
* NOT\_YET\_DEFINED:

## G826Type

Contains Enumeration Literals:

* ES:
  + Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::es .
* SES:
  + Severely Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::ses .
* CSES:
  + Consecutive Severely Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::cses .
* UAS:
  + Unavailable Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::unavailability.
* NOT\_SPECIFIED:

## GranularityPeriodType

The enumeration with the options for granularity period of the performance data.

Contains Enumeration Literals:

* UNKNOWN:
* PERIOD-15-MIN:
* PERIOD-24-HOURS:
* NOT\_YET\_DEFINED:

## InterfaceStatusType

Current Interface Status

Contains Enumeration Literals:

* UP:
  + Ready to pass packets.
* DOWN:
  + The interface does not pass any packets.
* TESTING:
  + In some test mode. No operational packets can be passed.
* UNKNOWN:
  + Status cannot be determined for some reason.
* DORMANT:
  + Waiting for some external event.
* NOT\_PRESENT:
  + Some component (typically hardware) is missing.
* LOWER\_LAYER\_DOWN:
  + Down due to state of lower-layer interface(s).
* ADMIN\_DOWN:
  + Down due to configuration.
* NOT\_YET\_DEFINED:

## LayerProtocolNameType

A controlled list of LayerProtocol names.

Contains Enumeration Literals:

* LAYER\_PROTOCOL\_NAME\_TYPE\_AIR\_LAYER:

## LoopBackType

Contains Enumeration Literals:

* RF\_TO\_REMOTE:
  + Returning the header information of the remote site back to the remote site on the radio interface between both outdoor units.
* RF\_TO\_LOCAL:
  + Returning the header information of the local site back to the local site on the radio interface between both outdoor units.
* IF\_TO\_REMOTE:
  + Returning the header information of the remote site back to the remote site on the intermediate frequency interface between local indoor unit and outdoor unit.
* IF\_TO\_LOCAL:
  + Returning the header information of the local site back to the local site on the intermediate frequency interface between local indoor unit and outdoor unit.
* NONE:

## OperationalStateType

The list of valid operational states for the connection.

Contains Enumeration Literals:

* ENABLED:
* DISABLED:
* NOT\_YET\_DEFINED:

## RadioSignalIdDatatypeType

Contains Enumeration Literals:

* INTEGER:
* STRING:
* NOT\_YET\_DEFINED:

## SeverityType

According to ITU-T M.3160

Contains Enumeration Literals:

* NON\_ALARMED:
* WARNING:
* MINOR:
* MAJOR:
* CRITICAL:
* NOT\_YET\_DEFINED:

## XLevelThresholdSecondKindType

According to ETSI EN 301 129 V1.1.2 (1999-05) chapter B.1.1

Contains Enumeration Literals:

* RLTS:
* TLTS:
* NOT\_YET\_DEFINED:

# Primitive Types